==============================================================
 ReadMe for Update of Baumer FWX and NCF driver for NeuroCheck
==============================================================
          ===/\ NeuroCheck 5.1 Service Pack 12 /\===

		  
If you are using a Baumer FWX NC Edition or a NCF camera in 
NeuroCheck 5.1 SP11 or earlier, the update to SP12 requires
also the update of the Baumer Sys driver.

Please proceed as follows:

1. Log on to your PC in a user profile with administrator rights.

2. Make sure that NeuroCheck is closed.

3. Update your previous NeuroCheck 5.1 installation to SP12
   by executing the self-extracting ZIP.

4. Copy the following files from the NcDriver folder into the 
   NeuroCheck installation folder (replace existing files):
   - NcFwBofx.DLL version 5.1.3047.0
   - NcFwBofx.chm 
   - FxLib.DLL version 5.1.0.8718
   - SysInfo.DLL version 5.1.0.8718

5. Open the Windows Device Manager (Control Panel > System > Hardware).
   
6. For each Baumer camera unter Baumer 1394 controlled devices
   open the Properties dialog and go to page Driver. Choose 
   Update Driver and search for the SysDriver folder provided with 
   this zip file. Install this driver (Baumer1394.sys version 2.10.0.0).
   Please note that Windows 7 need his own driver (version 2.20.0.0).
   
7. For a new installation of NCF cameras please install the Baumer 
   OHCI drivers as described in our Baumer FWX and NCF camera series 
   help file NcFwBofx.chm, page Installation, point 5.

8. Open NeuroCheck and verify if all cameras are detected correctly. 
   If not, then please reboot your PC.

# for further questions, please send an email to support@neurocheck.com

==================================================
Copyright (C) 2003 - 2010 NeuroCheck GmbH, Germany
==================================================


