=======================================================================
 Configuration files for Hilscher cifX fieldbus devices for NeuroCheck
=======================================================================
          ===/\ NeuroCheck 6.0 Service Pack 3 /\===


Normally that configuration files are not required to configure a 
Hilscher cifX fieldbus device, that is done in the configuration tool.

Due to the fact that the configuration tool doesn't support Windows 7 
you have to configure the inputs and outputs with pre-defined 
configuration files. Please note that the device driver supports 
Windows 7.

Please proceed as follows:

1. Run cifX Setup from Windows Control Panel (Small Icons view).

2. Select channel 0 of your cifX fieldbus device.
   If your board is not listed please check the installation and driver 
   versions.

3. Load firmware file if not done before (button Add). 
   The firmware files is provided in the directory <Firmware>.

4. Load configuration file (button Add). 
   The configuration files differ in station address and number of
   In- and Outputs.

5. Click Apply for file download.



# for further questions, please send an email to support@neurocheck.com

=======================================================================
              Copyright (C) 2011 NeuroCheck GmbH, Germany              
=======================================================================
Email: support@neurocheck.com
Web:   www.neurocheck.com




